***solution report.***

13 spectral bands: 443 nm– 2190 nm

(including 3 bands for atmospheric corrections)

> Spectral resolution: 15 nm– 180 nm

> Spatial resolution: 10 m, 20 m and 60 m

This is the most important part. We expect here not only solution description but also your proposals and result of research in different papers about soil erosion detection problem. In other words - what can help us to solve problem in the most effective way.